print, OFF
geom_in, ON

fluid_dynamics, ON
heat_eq, OFF
phase_change, OFF
vaporization, OFF
condensation, OFF
melting, OFF
solidification, OFF
surface_tension, ON
radiation, OFF
oxidation, OFF
temperature_dependency, OFF
multi_layer_no_coalescence, OFF,
vof_adv_fls, ON,
solute_diff, OFF,
eutectic, OFF,
LPT_calc, OFF
porous, OFF
laser, OFF
phasefield, OFF
wettability, OFF

WENO, ON
IBM, ON
interface_capturing_scheme, PLIC
heat_tvd3, OFF
visc_tvd3, OFF

vof_validate_init, OFF

bc_xm,    WALL
bc_xp,    WALL
bc_ym,    WALL
bc_yp,    WALL
bc_zm,    WALL
bc_zp,    OUT
bct_xm,   INSULATION
bct_xp,   INSULATION
bct_ym,   INSULATION
bct_yp,   INSULATION
bct_zm,   INSULATION
bct_zp,   INSULATION
bcrad_xm, INSULATION
bcrad_xp, INSULATION
bcrad_ym, INSULATION
bcrad_yp, INSULATION
bcrad_zm, INSULATION
bcrad_zp, INSULATION

binary, ON
gnuplot, OFF

fp, msgs/msgs.%04r.lst

output_mode, UNIFY_MPI
output_double, OFF

output_bnd_norm_u, ON
output_bnd_norm_v, ON
output_bnd_norm_w, ON
output_ll, ON
output_ls, ON
output_lls, ON
output_u, ON
output_v, ON
output_w, ON
output_p, ON
output_div_u, ON
output_data_directory, vdata, vdata
restart_data_directory, rdata, rdata
output_filename_templates, time/%c.%04n.dat, %c_%i/%c_%i_%04n.dat, %c/%c_%04n.dat
restart_filename_templates, %c.dat, %c_%i/%04r.dat, %c/%04r.dat
